;**************************************************************
;	Brother RJ-4030 Install Information.
;
;	Copyright (C) 1993-2012 Brother Industries, Ltd.
;
;	Don't modify this file.
;**************************************************************

[VERSION]
Ptsetup=1
OS=NT

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;;
;; [OSVERSION] Section
;;
;;  * Family = 9x or NT
;;      --- Specifies Target OS Environment.
;;
;;  * Major_From, * Major_Till, * Minor_From, * Minor_Till
;;      --- Specifies compatible OS version range.
;;           Win98 : Major=4 , Minor=10
;;           WinMe : Major=4 , Minor=90
;;           Win2k : Major=5 , Minor=0
;;           WinXP : Major=5 , Minor=1
;;      WinXP(x64) : Major=5 , Minor=2
;;          WS2003 : Major=5 , Minor=2
;;
;;  * IsDriverX64 = 1 or 0
;;      --- If it's the 64bit driver, set 1.
;;
;;  * BlockServer = 1 or 0
;;      --- Stop installation in the case of the Server type OS when the flag is 1.
;;
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
[OSVERSION]
Family=NT
Major_From =5
Minor_From =0
Major_Till =-1
Minor_Till =0
IsDriverX64=1
BlockServer=0


[PRINTER]
Version=300
;;;
Environment=Windows x64
DefaultDataType=NT EMF 1.008
;DefaultDataType=RAW
PrinterName=Brother RJ-4030
DriverName=Brother RJ-4030
PortMonitorName=0
;;;
DrvTopDir=.\Driver\x64
InfFileName=bsr403v.inf
CatFileName=bsr403v.cat

PnPID=VID_04F9&PID_2045
HardwareID=BrotherRJ-4030

;;; MUST!!
SetCOM=ViaFilePort

ModelID=bsr403

DeleteAtInstall=0


[PreDeletion]
IsDriverInbox=
DriverName=
LangMonName=
PortPreName=
InfName=
PnPID=VID_04F9&PID_2045
HardwareID=BrotherRJ-4030


[BAUDRATEWIZARD]
;;; (for MW with BT/SC-2000USB:)
;;;
SetPCBaudTool=ON
SetPCBaudPath=.\mwsetb.exe
SetPCBaudrate=115200

[PORT]
;;; Don't change:
PTCOM=ON
LPT=OFF
PTUSB=OFF

[LOGFILE]
DELETE=OFF
